

**Product Specifications / Technical Data**

Effective: January 2, 2019

|  |  |
| --- | --- |
| Composition: | Phthalate-Free  |
| Installation | Unilin Locking System |
| Size (inches / mm): | 7.08” x 48.03” (179.8 x 1219.9mm) |
| Gauge: | 4.0mm+1.0mm AcoustX G-Core Sound Absorbing Backing=5.0mm |
| Wear Layer: | 20mil (.5mm) |
| Finish: | Advanced Urethane Coating |
| Edge: | Painted Bevel |
| Sq.Ft. / Piece: | 2.36 |
| Sq.Ft. / Carton: | 23.63 |
| Pieces / Carton: | 10 |
| Cartons / Pallet: | 50 (1181.50 sq.ft.) |
| Pallets / 20’ Container: | 20 (23,630 sq.ft.) |
| Weight / Pallet: | 2,010lbs |
| Limited Warranty: | Lifetime Residential10 Year Commercial |
| **Testing** |
| ASTM F1700 – Product Classification: | Class III, Type B, Embossed SurfaceMeets and exceeds passing requirements |
| ASTM E648 – Radiant Panel (Critical Radiant Flux-Fire Rating Flaming Spread): | Meets and exceeds passing requirements (Class 1) |
| ASTM D2047 James Machine – Coefficient of Friction (Slip Resistance) | Meets and exceeds passing requirements |
| ASTM F925 – Resistance to Chemicals: | Meets and exceeds passing requirements |
| ASTM E492 – Impact Sound Insulation Acoustical Testing (IIC) | 58 IIC – over 6” concrete |
| ASTM F970 - Static Load Limit: | Meets and exceeds passing requirements |
| **Sustainability** |
| Recycled Content: | No |
| ISO 9001 – Quality Management System: | Meets and exceeds passing requirements |
| ISO 14001 – Environmental Management System: | Meets and exceeds passing requirements |
| FloorScore® Certified: | Yes |

[www.acrylxusa.com](http://www.acrylxusa.com)

1-855 3 RASKIN